**Work-in-progress pallet note**

**TMP.12 Ver 2.0**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Work in progress ID Card | | | | | | Production order no. | | 16J15 |
| Product Name | | | | Office table | | Drawing Code | 222 | |
| Part / component name | | | | Long frame | | Quantity in this pallet | 900 | |
| FSC □ | PEFC □ | FSC CW ⊠ | Non-cert □ | Others |  | Species | Acacia mangium | |
| Processed dimensions (mm): | | | | | 34 X 55 X 1500 | | | |
| Oversize dimensions (mm): | | | | | 38 X 58 X 1520 | | | |
| **Process. No.** | | **Starting Quantity** | | **Processing name** | **Processed Quantity** | **Rejected Quantity** | **Remarks** | |
| 1 | | 900 | | Planing | 900 | 0 |  | |
| 2 | | 900 | | Drilling | 899 | 1 |  | |
| 3 | | 899 | | Mortising |  |  |  | |
| 4 | |  | | Sanding |  |  |  | |
| 5 | |  | |  |  |  |  | |
| 6 | |  | |  |  |  |  | |
| 7 | |  | |  |  |  |  | |



Increasing capacity of CSOs and SMEs to implement FLEGT requirements. This project is partly funded by the European Union

This publication has been produced with the assistance of the European Union. The contents of this publication are the sole responsibility of NEPCon and can in no way be taken to reflect the views of the European Union.